# Thermal Printer Configuration

Back to Dashboard

##### Status

Connection Status
Loading...
Queue Size
0
Printed Jobs
0
Failed Jobs
0
Uptime
0s

##### Configuration

Enable Thermal Printer

###### Printer Connection

Printer Type
USB Vendor ID e.g., 0x04b8 for Epson (leave empty for auto-detect)
USB Product ID e.g., 0x0e15 for TM-T20 (leave empty for auto-detect)
Network Host/IP
Network Port

###### Event Filters

Print Chat Messages
Print Gifts
Print Follows
Print Shares
Minimum Coins to Print (Gifts) Only print gifts with at least this many coins (saves paper)
Ignore Bot Commands (messages starting with '!')

###### Formatting

Auto-cut paper after each event
Paper Width (characters) Typical: 48 for 80mm paper, 32 for 58mm paper
Character Encoding

###### Advanced Settings

Reconnect Attempts
Reconnect Delay (ms)
Max Queue Size
Print Delay (ms) Delay between print jobs (prevents overloading)